Stepper motor calibration

Driver: A3967

Microstepping =1/8 (already enabled by default)

Steps for one complete rotation = 1600

Steps for 1 degree rotation= 1600/360= 40/9

For translation with T8 threaded rod---

Pitch=8mm

1600 steps = 8mm

1mm=200 steps